From e1cf02a6e1a696a4eea5d0f4fa3c2f8ce1a45334 Mon Sep 17 00:00:00 2001
From: Cristian Ciocaltea <cristian.ciocaltea@collabora.com>
Date: Tue, 16 Jan 2024 03:13:38 +0200
Subject: [PATCH 433/463] arm64: dts: rockchip: Enable HDMI0 PHY clk provider
 on rk3588

The HDMI0 PHY can be used as a clock provider on RK3588, hence add the
missing #clock-cells property.
---
 arch/arm64/boot/dts/rockchip/rk3588-base.dtsi | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi b/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi
index 6b3a81650d964..3eb5f17a07ef8 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi
@@ -2696,6 +2696,7 @@ hdptxphy_hdmi0: phy@fed60000 {
 		reg = <0x0 0xfed60000 0x0 0x2000>;
 		clocks = <&cru CLK_USB2PHY_HDPTXRXPHY_REF>, <&cru PCLK_HDPTX0>;
 		clock-names = "ref", "apb";
+		#clock-cells = <0>;
 		#phy-cells = <0>;
 		resets = <&cru SRST_HDPTX0>, <&cru SRST_P_HDPTX0>,
 			 <&cru SRST_HDPTX0_INIT>, <&cru SRST_HDPTX0_CMN>,
-- 
2.46.0

