From 20c13b5ecd23cc744a25a1dc4bef52c5bc0931ac Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Mon, 13 Sep 2021 14:37:39 +0200
Subject: [PATCH 032/463] 8723cs: Fix compile warnings

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 drivers/staging/rtl8723cs/core/rtw_mlme_ext.c           | 4 ++--
 drivers/staging/rtl8723cs/hal/hal_intf.c                | 2 +-
 drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c | 2 +-
 3 files changed, 4 insertions(+), 4 deletions(-)

diff --git a/drivers/staging/rtl8723cs/core/rtw_mlme_ext.c b/drivers/staging/rtl8723cs/core/rtw_mlme_ext.c
index 07aab079179b9..11da273bee38a 100644
--- a/drivers/staging/rtl8723cs/core/rtw_mlme_ext.c
+++ b/drivers/staging/rtl8723cs/core/rtw_mlme_ext.c
@@ -298,7 +298,7 @@ void rtw_txpwr_init_regd(struct rf_ctl_t *rfctl)
 		);
 		if (rfctl->regd_name)
 			break;
-		/* fall through */
+		fallthrough;
 	default:
 		rfctl->regd_name = regd_str(TXPWR_LMT_WW);
 		RTW_PRINT("assign %s for default case\n", regd_str(TXPWR_LMT_WW));
@@ -1665,7 +1665,7 @@ void mgt_dispatcher(_adapter *padapter, union recv_frame *precv_frame)
 			ptable->func = &OnAuth;
 		else
 			ptable->func = &OnAuthClient;
-	/* fall through */
+		fallthrough;
 	case WIFI_ASSOCREQ:
 	case WIFI_REASSOCREQ:
 		_mgt_dispatcher(padapter, ptable, precv_frame);
diff --git a/drivers/staging/rtl8723cs/hal/hal_intf.c b/drivers/staging/rtl8723cs/hal/hal_intf.c
index 762d1ac08fcc0..c39b37b773a7f 100644
--- a/drivers/staging/rtl8723cs/hal/hal_intf.c
+++ b/drivers/staging/rtl8723cs/hal/hal_intf.c
@@ -1370,7 +1370,7 @@ s32 c2h_handler(_adapter *adapter, u8 id, u8 seq, u8 plen, u8 *payload)
 	case C2H_EXTEND:
 		sub_id = payload[0];
 		/* no handle, goto default */
-		/* fall through */
+		fallthrough;
 
 	default:
 		if (phydm_c2H_content_parsing(adapter_to_phydm(adapter), id, plen, payload) != TRUE)
diff --git a/drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c b/drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c
index 54424a82ce19d..ca999734af96c 100644
--- a/drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c
+++ b/drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c
@@ -6767,7 +6767,7 @@ static void rtw_get_chbwoff_from_cfg80211_chan_def(
 	switch (chandef->width) {
 	case NL80211_CHAN_WIDTH_20_NOHT:
 		*ht = 0;
-		/* fall through */
+		fallthrough;
 	case NL80211_CHAN_WIDTH_20:
 		*bw = CHANNEL_WIDTH_20;
 		*offset = HAL_PRIME_CHNL_OFFSET_DONT_CARE;
-- 
2.46.0

