From a7458e7e43bd82ee9cf29d1e066d5c6443251f33 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Thu, 4 Feb 2021 00:55:20 +0100
Subject: [PATCH 120/463] leds: axp20x: Support charger LED on AXP20x like
 PMICs

There is single LED that can be turned on and off by the user, or set to
be controlled by the charger in 2 different modes.

The driver initializes the LED to be controlled by the charger, but
allows to switch it to user control, and change the mode of charging
indication via a sysfs.

The driver was developed on AXP813, but should work on other PMICs like
that without changes.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 drivers/leds/Kconfig       |  15 +++
 drivers/leds/Makefile      |   1 +
 drivers/leds/leds-axp20x.c | 253 +++++++++++++++++++++++++++++++++++++
 drivers/mfd/axp20x.c       |   3 +
 4 files changed, 272 insertions(+)
 create mode 100644 drivers/leds/leds-axp20x.c

diff --git a/drivers/leds/Kconfig b/drivers/leds/Kconfig
index 8d9d8da376e46..24c8965cd4aeb 100644
--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -944,6 +944,14 @@ config LEDS_IP30
 	  To compile this driver as a module, choose M here: the module
 	  will be called leds-ip30.
 
+config LEDS_SGM3140
+	tristate "LED support for the SGM3140"
+	depends on LEDS_CLASS_FLASH
+	depends on V4L2_FLASH_LED_CLASS || !V4L2_FLASH_LED_CLASS
+	help
+	  This option enables support for the SGM3140 500mA Buck/Boost Charge
+	  Pump LED Driver.
+
 config LEDS_ACER_A500
 	tristate "Power button LED support for Acer Iconia Tab A500"
 	depends on LEDS_CLASS && MFD_ACER_A500_EC
@@ -951,6 +959,13 @@ config LEDS_ACER_A500
 	  This option enables support for the Power Button LED of
 	  Acer Iconia Tab A500.
 
+config LEDS_AXP20X
+	tristate "Charger LED support for AXP20X-like PMICs (AXP813, ...)"
+	depends on LEDS_CLASS && MFD_AXP20X
+	help
+	  This option enables support for on-chip LED driver on
+	  AXP20X-like PMICs.
+
 source "drivers/leds/blink/Kconfig"
 
 comment "Flash and Torch LED drivers"
diff --git a/drivers/leds/Makefile b/drivers/leds/Makefile
index 18afbb5a23ee5..fde9e39f0d532 100644
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -92,6 +92,7 @@ obj-$(CONFIG_LEDS_TURRIS_OMNIA)		+= leds-turris-omnia.o
 obj-$(CONFIG_LEDS_WM831X_STATUS)	+= leds-wm831x-status.o
 obj-$(CONFIG_LEDS_WM8350)		+= leds-wm8350.o
 obj-$(CONFIG_LEDS_WRAP)			+= leds-wrap.o
+obj-$(CONFIG_LEDS_AXP20X)		+= leds-axp20x.o
 
 # Kinetic ExpressWire Protocol
 obj-$(CONFIG_LEDS_EXPRESSWIRE)		+= leds-expresswire.o
diff --git a/drivers/leds/leds-axp20x.c b/drivers/leds/leds-axp20x.c
new file mode 100644
index 0000000000000..e2877af1032a7
--- /dev/null
+++ b/drivers/leds/leds-axp20x.c
@@ -0,0 +1,253 @@
+// SPDX-License-Identifier: GPL-2.0-or-later
+/*
+ * LED Driver for X-Powers AXP813 PMIC and similar.
+ *
+ * Copyright(c) 2020 Ondrej Jirman <megi@xff.cz>
+ */
+
+#include <linux/module.h>
+#include <linux/kernel.h>
+#include <linux/platform_device.h>
+#include <linux/leds.h>
+#include <linux/slab.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/mfd/axp20x.h>
+
+#define AXP20X_CHGLED_CTRL_MASK		BIT(3)
+#define AXP20X_CHGLED_CTRL_CHARGER	BIT(3)
+#define AXP20X_CHGLED_CTRL_USER		0
+
+#define AXP20X_CHRG_CTRL2_MODE		BIT(4)
+
+#define AXP20X_CHGLED_USER_STATE_MASK		GENMASK(5, 4)
+#define AXP20X_CHGLED_USER_STATE_OFF		(0 << 4)
+#define AXP20X_CHGLED_USER_STATE_BLINK_SLOW	(1 << 4)
+#define AXP20X_CHGLED_USER_STATE_BLINK_FAST	(2 << 4)
+#define AXP20X_CHGLED_USER_STATE_ON		(3 << 4)
+
+static struct led_hw_trigger_type axp20x_charger_led_trigger_type;
+
+struct axp20x_led {
+	struct led_classdev cdev;
+	struct regmap *regmap;
+};
+
+static int axp20x_led_set(struct led_classdev *led_cdev,
+			   enum led_brightness value)
+{
+	struct axp20x_led *led =
+			container_of(led_cdev, struct axp20x_led, cdev);
+	unsigned int val;
+
+	val = value == LED_OFF ? AXP20X_CHGLED_USER_STATE_OFF :
+		AXP20X_CHGLED_USER_STATE_ON;
+
+	return regmap_update_bits(led->regmap, AXP20X_OFF_CTRL,
+				  AXP20X_CHGLED_USER_STATE_MASK, val);
+
+}
+
+static int axp20x_set_charger_control(struct led_classdev *led_cdev, bool on)
+{
+	struct axp20x_led *led = container_of(led_cdev, struct axp20x_led, cdev);
+
+	return regmap_update_bits(led->regmap, AXP20X_OFF_CTRL,
+				  AXP20X_CHGLED_CTRL_MASK,
+				  on ? AXP20X_CHGLED_CTRL_CHARGER :
+				  AXP20X_CHGLED_CTRL_USER);
+}
+
+static int axp20x_trig_charger_activate(struct led_classdev *led_cdev)
+{
+	return axp20x_set_charger_control(led_cdev, true);
+}
+
+static void axp20x_trig_charger_deactivate(struct led_classdev *led_cdev)
+{
+	axp20x_set_charger_control(led_cdev, false);
+}
+
+static ssize_t charger_mode_show(struct device *dev,
+				 struct device_attribute *attr, char *buf)
+{
+	struct led_classdev *led_cdev = led_trigger_get_led(dev);
+	struct axp20x_led *led = container_of(led_cdev, struct axp20x_led, cdev);
+	unsigned int val;
+	int ret;
+
+	ret = regmap_read(led->regmap, AXP20X_CHRG_CTRL2, &val);
+	if (ret)
+		return ret;
+
+	return scnprintf(buf, PAGE_SIZE, "%u\n",
+			 val & AXP20X_CHRG_CTRL2_MODE ? 1 : 0);
+}
+
+static ssize_t charger_mode_store(struct device *dev,
+				  struct device_attribute *attr,
+				  const char *buf, size_t len)
+{
+	struct led_classdev *led_cdev = led_trigger_get_led(dev);
+	struct axp20x_led *led = container_of(led_cdev, struct axp20x_led, cdev);
+	unsigned int mode;
+	int ret;
+
+	ret = kstrtouint(buf, 0, &mode);
+	if (ret)
+		return ret;
+
+	if (mode > 1)
+		return -ERANGE;
+
+	ret = regmap_update_bits(led->regmap, AXP20X_CHRG_CTRL2,
+				 AXP20X_CHRG_CTRL2_MODE,
+				 mode ? AXP20X_CHRG_CTRL2_MODE : 0);
+	if (ret)
+		return ret;
+
+	return len;
+}
+static DEVICE_ATTR_RW(charger_mode);
+
+static struct attribute *axp20x_led_attrs[] = {
+	&dev_attr_charger_mode.attr,
+	NULL,
+};
+
+ATTRIBUTE_GROUPS(axp20x_led);
+
+static struct led_trigger axp20x_charger_led_trigger = {
+	.name		= "charger",
+	.trigger_type	= &axp20x_charger_led_trigger_type,
+	.activate	= axp20x_trig_charger_activate,
+	.deactivate	= axp20x_trig_charger_deactivate,
+	.groups		= axp20x_led_groups,
+};
+
+static int axp20x_led_probe(struct platform_device *pdev)
+{
+	struct axp20x_dev *axp20x;
+	struct axp20x_led *led;
+	unsigned int val;
+	int ret;
+
+	if (!of_device_is_available(pdev->dev.of_node))
+		return -ENODEV;
+
+	axp20x = dev_get_drvdata(pdev->dev.parent);
+	if (!axp20x)
+		return -EINVAL;
+
+	led = devm_kzalloc(&pdev->dev,
+			   sizeof(struct axp20x_led),
+			   GFP_KERNEL);
+	if (!led)
+		return -ENOMEM;
+
+	platform_set_drvdata(pdev, led);
+
+	led->regmap = axp20x->regmap;
+
+	led->cdev.name = "axp20x-chgarger-led";
+	led->cdev.brightness_set_blocking = axp20x_led_set;
+	led->cdev.brightness = LED_OFF;
+	led->cdev.max_brightness = 1;
+	led->cdev.trigger_type = &axp20x_charger_led_trigger_type;
+
+	ret = regmap_read(led->regmap, AXP20X_OFF_CTRL, &val);
+	if (ret) {
+		dev_err(&pdev->dev, "Failed to read charger control status\n");
+		return ret;
+	}
+
+	if ((val & AXP20X_CHGLED_CTRL_MASK) == AXP20X_CHGLED_CTRL_CHARGER)
+		led->cdev.default_trigger = axp20x_charger_led_trigger.name;
+
+	ret = devm_led_classdev_register(pdev->dev.parent, &led->cdev);
+	if (ret) {
+		dev_err(&pdev->dev, "Failed to register led %s\n",
+			led->cdev.name);
+		return ret;
+	}
+
+	ret = regmap_update_bits(led->regmap, AXP20X_OFF_CTRL,
+				 AXP20X_CHGLED_CTRL_MASK,
+				 AXP20X_CHGLED_CTRL_CHARGER);
+	if (ret) {
+		dev_err(&pdev->dev, "Failed to enable charger control\n");
+		return ret;
+	}
+
+	ret = axp20x_led_set(&led->cdev, led->cdev.brightness);
+	if (ret) {
+		dev_err(&pdev->dev, "Failed to init led brightness\n");
+		return ret;
+	}
+
+	return 0;
+}
+
+static void axp20x_led_shutdown(struct platform_device *pdev)
+{
+	struct axp20x_led *led = platform_get_drvdata(pdev);
+
+	/* On shutdown, we want to give LED control back to the PMIC,
+	 * so that it doesn't stay on, while the system is off.
+	 */
+
+	axp20x_led_set(&led->cdev, LED_OFF);
+	axp20x_set_charger_control(&led->cdev, true);
+}
+
+static void axp20x_led_remove(struct platform_device *pdev)
+{
+	axp20x_led_shutdown(pdev);
+}
+
+static const struct of_device_id axp20x_leds_of_match[] = {
+	{ .compatible = "x-powers,axp813-charger-led", },
+	{ },
+};
+MODULE_DEVICE_TABLE(of, axp20x_leds_of_match);
+
+static struct platform_driver axp20x_led_driver = {
+	.driver		= {
+		.name	= "leds-axp20x",
+		.of_match_table = axp20x_leds_of_match,
+	},
+	.probe		= axp20x_led_probe,
+	.remove		= axp20x_led_remove,
+	.shutdown	= axp20x_led_shutdown,
+};
+
+static int __init axp20x_led_driver_init(void)
+{
+	int ret;
+
+	ret = led_trigger_register(&axp20x_charger_led_trigger);
+	if (ret)
+		return ret;
+
+	ret = platform_driver_register(&axp20x_led_driver);
+	if (ret) {
+		led_trigger_unregister(&axp20x_charger_led_trigger);
+		return ret;
+	}
+
+	return 0;
+}
+
+static void __exit axp20x_led_driver_exit(void)
+{
+	platform_driver_unregister(&axp20x_led_driver);
+	led_trigger_unregister(&axp20x_charger_led_trigger);
+}
+
+module_init(axp20x_led_driver_init);
+module_exit(axp20x_led_driver_exit);
+
+MODULE_AUTHOR("Ondrej Jirman <megi@xff.cz>");
+MODULE_DESCRIPTION("LED driver for AXP813 PMIC");
+MODULE_LICENSE("GPL");
+MODULE_ALIAS("platform:leds-axp20x");
diff --git a/drivers/mfd/axp20x.c b/drivers/mfd/axp20x.c
index dacd3c96c9f57..d35b5cc6b8fe2 100644
--- a/drivers/mfd/axp20x.c
+++ b/drivers/mfd/axp20x.c
@@ -1172,6 +1172,9 @@ static const struct mfd_cell axp813_cells[] = {
 		.num_resources	= ARRAY_SIZE(axp803_usb_power_supply_resources),
 		.resources	= axp803_usb_power_supply_resources,
 		.of_compatible	= "x-powers,axp813-usb-power-supply",
+	}, {
+		.name		= "axp20x-charger-led",
+		.of_compatible	= "x-powers,axp813-charger-led",
 	},
 };
 
-- 
2.46.0

