From 577b20d4e32f10fa9f8fc1b2d8098f1feeb26fda Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Thu, 1 Aug 2024 14:04:59 +0200
Subject: [PATCH 424/463] arm64: dts: rockchip: rk3588-orangepi-5-plus: Add
 hdmi output support

Enable HDMI output on this board.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 .../dts/rockchip/rk3588-orangepi-5-plus.dts   | 52 +++++++++++++++++++
 1 file changed, 52 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
index 20e6e87f829d7..86d2e6900b776 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
@@ -9,6 +9,7 @@
 #include <dt-bindings/leds/common.h>
 #include <dt-bindings/input/input.h>
 #include <dt-bindings/pinctrl/rockchip.h>
+#include <dt-bindings/soc/rockchip,vop2.h>
 #include <dt-bindings/usb/pd.h>
 #include "rk3588.dtsi"
 
@@ -85,6 +86,17 @@ led {
 		};
 	};
 
+	hdmi0-con {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi0_con_in: endpoint {
+				remote-endpoint = <&hdmi0_out_con>;
+			};
+		};
+	};
+
 	fan: pwm-fan {
 		compatible = "pwm-fan";
 		cooling-levels = <0 70 75 80 100>;
@@ -275,6 +287,31 @@ &cpu_l3 {
 	cpu-supply = <&vdd_cpu_lit_s0>;
 };
 
+&display_subsystem {
+	clocks = <&hdptxphy_hdmi0>;
+	clock-names = "hdmi0_phy_pll";
+};
+
+&hdmi0 {
+	status = "okay";
+};
+
+&hdmi0_in {
+	hdmi0_in_vp0: endpoint {
+		remote-endpoint = <&vp0_out_hdmi0>;
+	};
+};
+
+&hdmi0_out {
+	hdmi0_out_con: endpoint {
+		remote-endpoint = <&hdmi0_con_in>;
+	};
+};
+
+&hdptxphy_hdmi0 {
+	status = "okay";
+};
+
 &i2c0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&i2c0m2_xfer>;
@@ -984,3 +1021,18 @@ usbdp_phy0_dp_altmode_mux: endpoint@1 {
 &usbdp_phy1 {
 	status = "okay";
 };
+
+&vop_mmu {
+	status = "okay";
+};
+
+&vop {
+	status = "okay";
+};
+
+&vp0 {
+	vp0_out_hdmi0: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
+		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
+		remote-endpoint = <&hdmi0_in_vp0>;
+	};
+};
-- 
2.46.0

