From c5d95be953a8c16853b191630baf60494be9d9a8 Mon Sep 17 00:00:00 2001
From: Cristian Ciocaltea <cristian.ciocaltea@collabora.com>
Date: Mon, 15 Jan 2024 22:47:41 +0200
Subject: [PATCH 431/463] arm64: dts: rockchip: Add HDMI0 bridge to rk3588

Add DT node for the HDMI0 bridge found on RK3588 SoC.

Signed-off-by: Cristian Ciocaltea <cristian.ciocaltea@collabora.com>
---
 arch/arm64/boot/dts/rockchip/rk3588-base.dtsi | 42 +++++++++++++++++++
 1 file changed, 42 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi b/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi
index ee99166ebd46f..6b3a81650d964 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi
@@ -1254,6 +1254,48 @@ i2s9_8ch: i2s@fddfc000 {
 		status = "disabled";
 	};
 
+	hdmi0: hdmi@fde80000 {
+		compatible = "rockchip,rk3588-dw-hdmi-qp";
+		reg = <0x0 0xfde80000 0x0 0x20000>;
+		clocks = <&cru PCLK_HDMITX0>,
+			 <&cru CLK_HDMITX0_EARC>,
+			 <&cru CLK_HDMITX0_REF>,
+			 <&cru MCLK_I2S5_8CH_TX>,
+			 <&cru CLK_HDMIHDP0>,
+			 <&cru HCLK_VO1>;
+		clock-names = "pclk", "earc", "ref", "aud", "hdp", "hclk_vo1";
+		interrupts = <GIC_SPI 169 IRQ_TYPE_LEVEL_HIGH 0>,
+			     <GIC_SPI 170 IRQ_TYPE_LEVEL_HIGH 0>,
+			     <GIC_SPI 171 IRQ_TYPE_LEVEL_HIGH 0>,
+			     <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH 0>,
+			     <GIC_SPI 360 IRQ_TYPE_LEVEL_HIGH 0>;
+		interrupt-names = "avp", "cec", "earc", "main", "hpd";
+		phys = <&hdptxphy_hdmi0>;
+		phy-names = "hdmi";
+		pinctrl-names = "default";
+		pinctrl-0 = <&hdmim0_tx0_cec &hdmim0_tx0_hpd
+			     &hdmim0_tx0_scl &hdmim0_tx0_sda>;
+		power-domains = <&power RK3588_PD_VO1>;
+		resets = <&cru SRST_HDMITX0_REF>, <&cru SRST_HDMIHDP0>;
+		reset-names = "ref", "hdp";
+		rockchip,grf = <&sys_grf>;
+		rockchip,vo1_grf = <&vo1_grf>;
+		status = "disabled";
+
+		ports {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			hdmi0_in: port@0 {
+				reg = <0>;
+			};
+
+			hdmi0_out: port@1 {
+				reg = <1>;
+			};
+		};
+	};
+
 	qos_gpu_m0: qos@fdf35000 {
 		compatible = "rockchip,rk3588-qos", "syscon";
 		reg = <0x0 0xfdf35000 0x0 0x20>;
-- 
2.46.0

