From 618de3be4f7280f8b1433c775715577f6b1784df Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sat, 1 Feb 2020 23:41:18 +0100
Subject: [PATCH 219/463] arm64: dts: sun50i-a64: Set fifo-size for uarts

Boot time optimization.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index e868ca5ae753a..59985e09410c5 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -980,6 +980,7 @@ uart0: serial@1c28000 {
 			interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART0>;
 			resets = <&ccu RST_BUS_UART0>;
 			status = "disabled";
@@ -991,6 +992,7 @@ uart1: serial@1c28400 {
 			interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART1>;
 			resets = <&ccu RST_BUS_UART1>;
 			status = "disabled";
@@ -1002,6 +1004,7 @@ uart2: serial@1c28800 {
 			interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART2>;
 			resets = <&ccu RST_BUS_UART2>;
 			status = "disabled";
@@ -1013,6 +1016,7 @@ uart3: serial@1c28c00 {
 			interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART3>;
 			resets = <&ccu RST_BUS_UART3>;
 			status = "disabled";
@@ -1024,6 +1028,7 @@ uart4: serial@1c29000 {
 			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART4>;
 			resets = <&ccu RST_BUS_UART4>;
 			status = "disabled";
-- 
2.46.0

