From 78d87e387777c4343f31a52e0dcbed8b68ebc51c Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Tue, 20 Aug 2019 14:54:48 +0200
Subject: [PATCH 144/463] arm64: dts: allwinner: orange-pi-3: Enable ethernet

Orange Pi 3 has two regulators that power the Realtek RTL8211E
PHY. According to the datasheet, both regulators need to be enabled
at the same time, or that "phy-io" should be enabled slightly earlier
than "phy" regulator.

RTL8211E/RTL8211EG datasheet says:

  Note 4: 2.5V (or 1.8/1.5V) RGMII power should be risen simultaneously
  or slightly earlier than 3.3V power. Rising 2.5V (or 1.8/1.5V) power
  later than 3.3V power may lead to errors.

The driver ensures the regulator enable ordering. The timing is set
in DT via startup-delay-us.

We also need to wait at least 30ms after power-up/reset, before
accessing the PHY registers.

All values of RX/TX delay were tested exhaustively and a middle one
of the range of working values was chosen.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 .../dts/allwinner/sun50i-h6-orangepi-3.dts    | 40 +++++++++++++++++++
 1 file changed, 40 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
index 6c3bfe3d09d9a..f32f95c8ed5e3 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
@@ -15,6 +15,7 @@ / {
 	aliases {
 		serial0 = &uart0;
 		serial1 = &uart1;
+		ethernet0 = &emac;
 	};
 
 	chosen {
@@ -64,6 +65,15 @@ reg_vcc5v: vcc5v {
 		regulator-always-on;
 	};
 
+	reg_gmac_2v5: gmac-2v5 {
+		compatible = "regulator-fixed";
+		regulator-name = "gmac-2v5";
+		regulator-min-microvolt = <2500000>;
+		regulator-max-microvolt = <2500000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>; /* PD6 */
+	};
+
 	reg_vcc33_wifi: vcc33-wifi {
 		/* Always on 3.3V regulator for WiFi and BT */
 		compatible = "regulator-fixed";
@@ -128,6 +138,35 @@ hdmi_out_con: endpoint {
 	};
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&ext_rgmii_pins>;
+	phy-mode = "rgmii-id";
+	phy-handle = <&ext_rgmii_phy>;
+	/*
+	 * The board uses 2.5V RGMII signalling. Power sequence to enable
+	 * the phy is to enable GMAC-2V5 and GMAC-3V (aldo2) power rails
+	 * at the same time and to wait 100ms. The driver enables phy-io
+	 * first. Delay is achieved with enable-ramp-delay on reg_aldo2.
+	 */
+	phy-supply = <&reg_aldo2>;
+	phy-io-supply = <&reg_gmac_2v5>;
+	allwinner,rx-delay-ps = <200>;
+	allwinner,tx-delay-ps = <200>;
+	status = "okay";
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+
+		reset-gpios = <&pio 3 14 GPIO_ACTIVE_LOW>; /* PD14 */
+		reset-assert-us = <15000>;
+		reset-deassert-us = <40000>;
+	};
+};
+
 &mmc0 {
 	vmmc-supply = <&reg_cldo1>;
 	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
@@ -211,6 +250,7 @@ reg_aldo2: aldo2 {
 				regulator-min-microvolt = <3300000>;
 				regulator-max-microvolt = <3300000>;
 				regulator-name = "vcc33-audio-tv-ephy-mac";
+				regulator-enable-ramp-delay = <100000>;
 			};
 
 			/* ALDO3 is shorted to CLDO1 */
-- 
2.46.0

