From 057cbe543940460278954a63bc12859cd941f81f Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Tue, 23 Jun 2020 19:15:37 +0200
Subject: [PATCH 104/463] ARM: dts: sun8i-a83t-tbs-a711: Add regulators to the
 accelerometer

The bosch,bma250 driver will fail to probe if the regulators are
not specified in DT, because it tries to set voltage on dummy
regulators, which fails with EINVAL.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
index 925891a1d6d9f..ce1a8d98b5483 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
@@ -268,6 +268,8 @@ accelerometer@18 {
 		reg = <0x18>;
 		interrupt-parent = <&pio>;
 		interrupts = <7 10 IRQ_TYPE_EDGE_RISING>; /* PH10 / EINT10 */
+		vdd-supply = <&reg_dcdc1>;
+		vddio-supply = <&reg_dcdc1>;
 	};
 
 	/* NFC (NPC 100) */
-- 
2.46.0

