From 88ec5287f8d75364611649618c5b53eb8bad9026 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Fri, 8 Dec 2017 12:44:22 +0100
Subject: [PATCH 109/463] ARM: dts: sun8i-a83t-tbs-a711: Increase voltage on
 the vibrator

Vibrator motor is weak at the current voltage. Increase the voltage.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
index f59cc4094f565..3c115862dca88 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
@@ -434,8 +434,8 @@ &reg_ldo_io0 {
 };
 
 &reg_ldo_io1 {
-	regulator-min-microvolt = <3100000>;
-	regulator-max-microvolt = <3100000>;
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
 	regulator-name = "vcc-vb";
 	status = "okay";
 };
-- 
2.46.0

