From 22c329e6c0a61c33deb44a324de595ca7c039cfd Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Wed, 25 Nov 2020 07:11:27 +0100
Subject: [PATCH 016/463] 8723cs: Modify makefile options to better suit
 PinePhone/Allwinner

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 drivers/staging/rtl8723cs/Makefile | 16 +++++++++-------
 1 file changed, 9 insertions(+), 7 deletions(-)

diff --git a/drivers/staging/rtl8723cs/Makefile b/drivers/staging/rtl8723cs/Makefile
index 7105db9b41fe2..b66d4e63c8881 100644
--- a/drivers/staging/rtl8723cs/Makefile
+++ b/drivers/staging/rtl8723cs/Makefile
@@ -1,6 +1,6 @@
 # SPDX-License-Identifier: GPL-2.0
 EXTRA_CFLAGS += $(USER_EXTRA_CFLAGS)
-EXTRA_CFLAGS += -O1
+EXTRA_CFLAGS += -O2
 #EXTRA_CFLAGS += -O3
 #EXTRA_CFLAGS += -Wall
 #EXTRA_CFLAGS += -Wextra
@@ -62,7 +62,7 @@ CONFIG_USB_AUTOSUSPEND = n
 CONFIG_HW_PWRP_DETECTION = n
 CONFIG_BT_COEXIST = y
 CONFIG_WAPI_SUPPORT = n
-CONFIG_EFUSE_CONFIG_FILE = y
+CONFIG_EFUSE_CONFIG_FILE = n
 CONFIG_EXT_CLK = n
 CONFIG_TRAFFIC_PROTECT = n
 CONFIG_LOAD_PHY_PARA_FROM_FILE = y
@@ -93,16 +93,16 @@ CONFIG_RTW_UP_MAPPING_RULE = tos
 CONFIG_RTW_MBO = n
 ########################## Android ###########################
 # CONFIG_RTW_ANDROID - 0: no Android, 4/5/6/7/8/9/10 : Android version
-CONFIG_RTW_ANDROID = 10
+CONFIG_RTW_ANDROID = 0
 
 ifeq ($(shell test $(CONFIG_RTW_ANDROID) -gt 0; echo $$?), 0)
 EXTRA_CFLAGS += -DCONFIG_RTW_ANDROID=$(CONFIG_RTW_ANDROID)
 endif
 ########################## Debug ###########################
-CONFIG_RTW_DEBUG = y
+CONFIG_RTW_DEBUG = n
 # default log level is _DRV_INFO_ = 4,
 # please refer to "How_to_set_driver_debug_log_level.doc" to set the available level.
-CONFIG_RTW_LOG_LEVEL = 2
+CONFIG_RTW_LOG_LEVEL = 6
 
 # enable /proc/net/rtlxxxx/ debug interfaces
 CONFIG_PROC_DEBUG = y
@@ -135,7 +135,7 @@ CONFIG_LAYER2_ROAMING = y
 #bit0: ROAM_ON_EXPIRED, #bit1: ROAM_ON_RESUME, #bit2: ROAM_ACTIVE
 CONFIG_ROAMING_FLAG = 0x3
 ###################### Platform Related #######################
-CONFIG_PLATFORM_I386_PC = n
+CONFIG_PLATFORM_I386_PC = y
 CONFIG_PLATFORM_ANDROID_X86 = n
 CONFIG_PLATFORM_ANDROID_INTEL_X86 = n
 CONFIG_PLATFORM_JB_X86 = n
@@ -160,7 +160,7 @@ CONFIG_PLATFORM_ARM_TCC8920_JB42 = n
 CONFIG_PLATFORM_ARM_TCC8930_JB42 = n
 CONFIG_PLATFORM_ARM_RK2818 = n
 CONFIG_PLATFORM_ARM_RK3066 = n
-CONFIG_PLATFORM_ARM_RK3188 = y
+CONFIG_PLATFORM_ARM_RK3188 = n
 CONFIG_PLATFORM_ARM_URBETTER = n
 CONFIG_PLATFORM_ARM_TI_PANDA = n
 CONFIG_PLATFORM_MIPS_JZ4760 = n
@@ -1332,6 +1332,8 @@ endif
 ifeq ($(CONFIG_PLATFORM_I386_PC), y)
 EXTRA_CFLAGS += -DCONFIG_LITTLE_ENDIAN
 EXTRA_CFLAGS += -DCONFIG_IOCTL_CFG80211 -DRTW_USE_CFG80211_STA_EVENT
+EXTRA_CFLAGS += -DCONFIG_CONCURRENT_MODE
+EXTRA_CFLAGS += -DCONFIG_RADIO_WORK
 
 SUBARCH := $(shell uname -m | sed -e s/i.86/i386/)
 ARCH ?= $(SUBARCH)
-- 
2.46.0

