From c2f82fc30bc3db9ae8abb1e99ce03984c82f76e9 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Sun, 30 Apr 2023 18:35:08 +0200
Subject: [PATCH 356/463] sdhci: arasan: Add runtime PM support

Add runtime PM support in Arasan SDHCI driver.

Signed-off-by: Manish Narani <manish.narani@xilinx.com>
---
 drivers/mmc/host/sdhci-of-arasan.c | 88 +++++++++++++++++++++++++++++-
 1 file changed, 86 insertions(+), 2 deletions(-)

diff --git a/drivers/mmc/host/sdhci-of-arasan.c b/drivers/mmc/host/sdhci-of-arasan.c
index 5edd024347bd5..05ab9c2ed0a46 100644
--- a/drivers/mmc/host/sdhci-of-arasan.c
+++ b/drivers/mmc/host/sdhci-of-arasan.c
@@ -20,6 +20,7 @@
 #include <linux/module.h>
 #include <linux/of.h>
 #include <linux/platform_device.h>
+#include <linux/pm_runtime.h>
 #include <linux/phy/phy.h>
 #include <linux/regmap.h>
 #include <linux/reset.h>
@@ -29,6 +30,7 @@
 #include "sdhci-cqhci.h"
 #include "sdhci-pltfm.h"
 
+#define SDHCI_ARASAN_AUTOSUSPEND_DELAY	2000 /* ms */
 #define SDHCI_ARASAN_VENDOR_REGISTER	0x78
 
 #define SDHCI_ARASAN_ITAPDLY_REGISTER	0xF0F8
@@ -563,6 +565,70 @@ static const struct sdhci_pltfm_data sdhci_arasan_cqe_pdata = {
 			SDHCI_QUIRK2_CLOCK_DIV_ZERO_BROKEN,
 };
 
+#ifdef CONFIG_PM
+static int sdhci_arasan_runtime_suspend(struct device *dev)
+{
+	struct platform_device *pdev = to_platform_device(dev);
+	struct sdhci_host *host = platform_get_drvdata(pdev);
+	struct sdhci_pltfm_host *pltfm_host = sdhci_priv(host);
+	struct sdhci_arasan_data *sdhci_arasan = sdhci_pltfm_priv(pltfm_host);
+	int ret;
+
+	if (sdhci_arasan->has_cqe) {
+		ret = cqhci_suspend(host->mmc);
+		if (ret)
+			return ret;
+	}
+
+	ret = sdhci_runtime_suspend_host(host);
+	if (ret)
+		return ret;
+
+	if (host->tuning_mode != SDHCI_TUNING_MODE_3)
+		mmc_retune_needed(host->mmc);
+
+	clk_disable(pltfm_host->clk);
+	clk_disable(sdhci_arasan->clk_ahb);
+
+	return 0;
+}
+
+static int sdhci_arasan_runtime_resume(struct device *dev)
+{
+	struct platform_device *pdev = to_platform_device(dev);
+	struct sdhci_host *host = platform_get_drvdata(pdev);
+	struct sdhci_pltfm_host *pltfm_host = sdhci_priv(host);
+	struct sdhci_arasan_data *sdhci_arasan = sdhci_pltfm_priv(pltfm_host);
+	int ret;
+
+	ret = clk_enable(sdhci_arasan->clk_ahb);
+	if (ret) {
+		dev_err(dev, "Cannot enable AHB clock.\n");
+		return ret;
+	}
+
+	ret = clk_enable(pltfm_host->clk);
+	if (ret) {
+		dev_err(dev, "Cannot enable SD clock.\n");
+		return ret;
+	}
+
+	ret = sdhci_runtime_resume_host(host, 0);
+	if (ret)
+		goto out;
+
+	if (sdhci_arasan->has_cqe)
+		return cqhci_resume(host->mmc);
+
+	return 0;
+out:
+	clk_disable(pltfm_host->clk);
+	clk_disable(sdhci_arasan->clk_ahb);
+
+	return ret;
+}
+#endif /* ! CONFIG_PM */
+
 #ifdef CONFIG_PM_SLEEP
 /**
  * sdhci_arasan_suspend - Suspend method for the driver
@@ -659,8 +725,10 @@ static int sdhci_arasan_resume(struct device *dev)
 }
 #endif /* ! CONFIG_PM_SLEEP */
 
-static SIMPLE_DEV_PM_OPS(sdhci_arasan_dev_pm_ops, sdhci_arasan_suspend,
-			 sdhci_arasan_resume);
+static const struct dev_pm_ops sdhci_arasan_dev_pm_ops = {
+	SET_SYSTEM_SLEEP_PM_OPS(sdhci_arasan_suspend, sdhci_arasan_resume)
+	SET_RUNTIME_PM_OPS(sdhci_arasan_runtime_suspend,
+			   sdhci_arasan_runtime_resume, NULL) };
 
 /**
  * sdhci_arasan_sdcardclk_recalc_rate - Return the card clock rate
@@ -1996,13 +2064,25 @@ static int sdhci_arasan_probe(struct platform_device *pdev)
 	if (of_device_is_compatible(np, "xlnx,versal-net-emmc"))
 		sdhci_arasan->internal_phy_reg = true;
 
+	pm_runtime_get_noresume(&pdev->dev);
+	pm_runtime_set_active(&pdev->dev);
+	pm_runtime_enable(&pdev->dev);
+	pm_runtime_set_autosuspend_delay(&pdev->dev,
+					 SDHCI_ARASAN_AUTOSUSPEND_DELAY);
+	pm_runtime_use_autosuspend(&pdev->dev);
+
 	ret = sdhci_arasan_add_host(sdhci_arasan);
 	if (ret)
 		goto err_add_host;
 
+	pm_runtime_put_autosuspend(&pdev->dev);
+
 	return 0;
 
 err_add_host:
+	pm_runtime_disable(&pdev->dev);
+	pm_runtime_set_suspended(&pdev->dev);
+	pm_runtime_put_noidle(&pdev->dev);
 	if (!IS_ERR(sdhci_arasan->phy))
 		phy_exit(sdhci_arasan->phy);
 unreg_clk:
@@ -2030,6 +2110,10 @@ static void sdhci_arasan_remove(struct platform_device *pdev)
 		phy_exit(sdhci_arasan->phy);
 	}
 
+	pm_runtime_get_sync(&pdev->dev);
+	pm_runtime_disable(&pdev->dev);
+	pm_runtime_put_noidle(&pdev->dev);
+
 	sdhci_arasan_unregister_sdclk(&pdev->dev);
 
 	sdhci_pltfm_remove(pdev);
-- 
2.46.0

