From 1a83a6ffd28c7f1163fea198352ec22387a0bc28 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Wed, 2 Dec 2020 12:45:21 +0100
Subject: [PATCH 024/463] 8723cs: Set CONFIG_RTW_SDIO_PM_KEEP_POWER = n to fix
 suspend (-38)

Device mmc1:0001:1 failed to suspend async: error -38

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 drivers/staging/rtl8723cs/Makefile | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/drivers/staging/rtl8723cs/Makefile b/drivers/staging/rtl8723cs/Makefile
index 5ef5557e58b72..0fe39a873866b 100644
--- a/drivers/staging/rtl8723cs/Makefile
+++ b/drivers/staging/rtl8723cs/Makefile
@@ -108,7 +108,7 @@ CONFIG_RTW_LOG_LEVEL = 6
 CONFIG_PROC_DEBUG = y
 
 ######################## Wake On Lan ##########################
-CONFIG_WOWLAN = y
+CONFIG_WOWLAN = n
 #bit3: ARP enable, bit2: deauth, bit1: unicast, bit0: magic pkt.
 CONFIG_WAKEUP_TYPE = 0xf
 CONFIG_WOW_LPS_MODE = default
@@ -127,7 +127,7 @@ CONFIG_PNO_SUPPORT = n
 CONFIG_PNO_SET_DEBUG = n
 CONFIG_AP_WOWLAN = n
 ######### Notify SDIO Host Keep Power During Syspend ##########
-CONFIG_RTW_SDIO_PM_KEEP_POWER = y
+CONFIG_RTW_SDIO_PM_KEEP_POWER = n
 ###################### MP HW TX MODE FOR VHT #######################
 CONFIG_MP_VHT_HW_TX_MODE = n
 ###################### ROAMING #####################################
-- 
2.46.0

