From e3d07420d87a67d442fca76f65bc7ed3b6505038 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Tue, 27 Aug 2024 14:11:46 +0200
Subject: [PATCH 405/463] arm64: dts: rk3399-pinephone-pro: Add wcam
 link-frequesncies

Suggested by luigi311.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts b/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
index 41024de7d4411..5bdd999052d5b 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
@@ -993,6 +993,7 @@ port {
 			wcam_out: endpoint {
 				remote-endpoint = <&mipi_in_wcam>;
 				data-lanes = <1 2 3 4>;
+                                link-frequencies = /bits/ 64 <636000000>;
 			};
 		};
 	};
-- 
2.46.0

