From 038e1fb95607a1055e79394e6b29f3293f50e72a Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Wed, 5 Aug 2020 11:19:01 +0200
Subject: [PATCH 170/463] arm64: dts: sun50i-a64-pinephone: Fix BH modem
 manager behavior

PP 1.1 has STATUS line multiplexed with POWER KEY, but reading it doesn't
work reliably. Just treat 1.1 as if it was 1.0, and ignore the STATUS.
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts
index 93dc8512fe458..d67f31ef529ee 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts
@@ -123,8 +123,8 @@ modem {
 
 		enable-gpios = <&pio 7 8 GPIO_ACTIVE_LOW>; /* PH8 */
 		reset-gpios = <&pio 2 4 GPIO_ACTIVE_HIGH>; /* PC4 */
-		status-gpios = <&pio 1 3 GPIO_ACTIVE_HIGH>; /* PB3 */
-		status-pwrkey-multiplexed; /* status acts as pwrkey */
+		pwrkey-gpios = <&pio 1 3 GPIO_ACTIVE_HIGH>; /* PB3 */
+		//status-pwrkey-multiplexed; /* status acts as pwrkey */
 
 		sleep-gpios = <&pio 7 7 GPIO_ACTIVE_HIGH>; /* PH7 */
 		wakeup-gpios = <&pio 1 2 GPIO_ACTIVE_HIGH>; /* PB2-RI */
-- 
2.46.0

