From 538d4b28990b198f6570eac2a5f206692aa01827 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sun, 12 Nov 2017 19:03:39 +0100
Subject: [PATCH 101/463] ARM: dts: suni-a83t: Add i2s0 pins

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi b/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi
index ed3d8e692d842..ef62ced26684b 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi
@@ -829,6 +829,11 @@ spdif_tx_pin: spdif-tx-pin {
 				function = "spdif";
 			};
 
+			i2s0_pins: i2s0-pins {
+				pins = "PB4", "PB5", "PB6", "PB7", "PB8";
+				function = "i2s0";
+			};
+
 			uart0_pb_pins: uart0-pb-pins {
 				pins = "PB9", "PB10";
 				function = "uart0";
-- 
2.46.0

