From faf3d06cdc3972c1f68dbcb40378c8d8706dee88 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sat, 1 Feb 2020 23:41:47 +0100
Subject: [PATCH 222/463] ARM: dts: sun8i-a83t: Set fifo-size for uarts

Boot time optimization.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi b/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi
index addf0cb0f465d..a21b1df98d13b 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/allwinner/sun8i-a83t.dtsi
@@ -933,6 +933,7 @@ uart0: serial@1c28000 {
 			interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART0>;
 			resets = <&ccu RST_BUS_UART0>;
 			status = "disabled";
@@ -944,6 +945,7 @@ uart1: serial@1c28400 {
 			interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART1>;
 			resets = <&ccu RST_BUS_UART1>;
 			status = "disabled";
@@ -955,6 +957,7 @@ uart2: serial@1c28800 {
 			interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART2>;
 			resets = <&ccu RST_BUS_UART2>;
 			status = "disabled";
@@ -966,6 +969,7 @@ uart3: serial@1c28c00 {
 			interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART3>;
 			resets = <&ccu RST_BUS_UART3>;
 			status = "disabled";
@@ -977,6 +981,7 @@ uart4: serial@1c29000 {
 			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
+			fifo-size = <64>;
 			clocks = <&ccu CLK_BUS_UART4>;
 			resets = <&ccu RST_BUS_UART4>;
 			status = "disabled";
-- 
2.46.0

