From d0df285c657d750ffb80eb5baa1152a9b0071c91 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Mon, 13 Sep 2021 14:38:17 +0200
Subject: [PATCH 033/463] 8723cs: Port to 5.15

Cut out apple talk protocol handling.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 drivers/staging/rtl8723cs/core/rtw_br_ext.c | 273 --------------------
 1 file changed, 273 deletions(-)

diff --git a/drivers/staging/rtl8723cs/core/rtw_br_ext.c b/drivers/staging/rtl8723cs/core/rtw_br_ext.c
index 9a0effd8b7eab..4251b825c8aeb 100644
--- a/drivers/staging/rtl8723cs/core/rtw_br_ext.c
+++ b/drivers/staging/rtl8723cs/core/rtw_br_ext.c
@@ -17,8 +17,6 @@
 #ifdef __KERNEL__
 	#include <linux/if_arp.h>
 	#include <net/ip.h>
-	#include <net/ipx.h>
-	#include <linux/atalk.h>
 	#include <linux/udp.h>
 	#include <linux/if_pppox.h>
 #endif
@@ -57,8 +55,6 @@
 
 #define NAT25_IPV4		01
 #define NAT25_IPV6		02
-#define NAT25_IPX		03
-#define NAT25_APPLE		04
 #define NAT25_PPPOE		05
 
 #define RTL_RELAY_TAG_LEN (ETH_ALEN)
@@ -73,8 +69,6 @@
            0    1    2    3    4    5    6    7    8    9   10
         |----|----|----|----|----|----|----|----|----|----|----|
   IPv4  |type|                             |      IP addr      |
-  IPX   |type|      Net addr     |          Node addr          |
-  IPX   |type|      Net addr     |Sckt addr|
   Apple |type| Network |node|
   PPPoE |type|   SID   |           AC MAC            |
 -----------------------------------------------------------------*/
@@ -169,39 +163,6 @@ static __inline__ void __nat25_generate_ipv4_network_addr(unsigned char *network
 }
 
 
-static __inline__ void __nat25_generate_ipx_network_addr_with_node(unsigned char *networkAddr,
-		unsigned int *ipxNetAddr, unsigned char *ipxNodeAddr)
-{
-	memset(networkAddr, 0, MAX_NETWORK_ADDR_LEN);
-
-	networkAddr[0] = NAT25_IPX;
-	memcpy(networkAddr + 1, (unsigned char *)ipxNetAddr, 4);
-	memcpy(networkAddr + 5, ipxNodeAddr, 6);
-}
-
-
-static __inline__ void __nat25_generate_ipx_network_addr_with_socket(unsigned char *networkAddr,
-		unsigned int *ipxNetAddr, unsigned short *ipxSocketAddr)
-{
-	memset(networkAddr, 0, MAX_NETWORK_ADDR_LEN);
-
-	networkAddr[0] = NAT25_IPX;
-	memcpy(networkAddr + 1, (unsigned char *)ipxNetAddr, 4);
-	memcpy(networkAddr + 5, (unsigned char *)ipxSocketAddr, 2);
-}
-
-
-static __inline__ void __nat25_generate_apple_network_addr(unsigned char *networkAddr,
-		unsigned short *network, unsigned char *node)
-{
-	memset(networkAddr, 0, MAX_NETWORK_ADDR_LEN);
-
-	networkAddr[0] = NAT25_APPLE;
-	memcpy(networkAddr + 1, (unsigned char *)network, 2);
-	networkAddr[3] = *node;
-}
-
-
 static __inline__ void __nat25_generate_pppoe_network_addr(unsigned char *networkAddr,
 		unsigned char *ac_mac, unsigned short *sid)
 {
@@ -329,19 +290,6 @@ static __inline__ int __nat25_network_hash(unsigned char *networkAddr)
 
 		x = networkAddr[7] ^ networkAddr[8] ^ networkAddr[9] ^ networkAddr[10];
 
-		return x & (NAT25_HASH_SIZE - 1);
-	} else if (networkAddr[0] == NAT25_IPX) {
-		unsigned long x;
-
-		x = networkAddr[1] ^ networkAddr[2] ^ networkAddr[3] ^ networkAddr[4] ^ networkAddr[5] ^
-		    networkAddr[6] ^ networkAddr[7] ^ networkAddr[8] ^ networkAddr[9] ^ networkAddr[10];
-
-		return x & (NAT25_HASH_SIZE - 1);
-	} else if (networkAddr[0] == NAT25_APPLE) {
-		unsigned long x;
-
-		x = networkAddr[1] ^ networkAddr[2] ^ networkAddr[3];
-
 		return x & (NAT25_HASH_SIZE - 1);
 	} else if (networkAddr[0] == NAT25_PPPOE) {
 		unsigned long x;
@@ -889,227 +837,6 @@ int nat25_db_handle(_adapter *priv, struct sk_buff *skb, int method)
 		}
 	}
 
-	/*---------------------------------------------------*/
-	/*         Handle IPX and Apple Talk frame          */
-	/*---------------------------------------------------*/
-	else if ((protocol == __constant_htons(ETH_P_IPX)) ||
-		 (protocol == __constant_htons(ETH_P_ATALK)) ||
-		 (protocol == __constant_htons(ETH_P_AARP))) {
-		unsigned char ipx_header[2] = {0xFF, 0xFF};
-		struct ipxhdr	*ipx = NULL;
-		struct elapaarp	*ea = NULL;
-		struct ddpehdr	*ddp = NULL;
-		unsigned char *framePtr = skb->data + ETH_HLEN;
-
-		if (protocol == __constant_htons(ETH_P_IPX)) {
-			RTW_INFO("NAT25: Protocol=IPX (Ethernet II)\n");
-			ipx = (struct ipxhdr *)framePtr;
-		} else { /* if(protocol <= __constant_htons(ETH_FRAME_LEN)) */
-			if (!memcmp(ipx_header, framePtr, 2)) {
-				RTW_INFO("NAT25: Protocol=IPX (Ethernet 802.3)\n");
-				ipx = (struct ipxhdr *)framePtr;
-			} else {
-				unsigned char ipx_8022_type =  0xE0;
-				unsigned char snap_8022_type = 0xAA;
-
-				if (*framePtr == snap_8022_type) {
-					unsigned char ipx_snap_id[5] = {0x0, 0x0, 0x0, 0x81, 0x37};		/* IPX SNAP ID */
-					unsigned char aarp_snap_id[5] = {0x00, 0x00, 0x00, 0x80, 0xF3};	/* Apple Talk AARP SNAP ID */
-					unsigned char ddp_snap_id[5] = {0x08, 0x00, 0x07, 0x80, 0x9B};	/* Apple Talk DDP SNAP ID */
-
-					framePtr += 3;	/* eliminate the 802.2 header */
-
-					if (!memcmp(ipx_snap_id, framePtr, 5)) {
-						framePtr += 5;	/* eliminate the SNAP header */
-
-						RTW_INFO("NAT25: Protocol=IPX (Ethernet SNAP)\n");
-						ipx = (struct ipxhdr *)framePtr;
-					} else if (!memcmp(aarp_snap_id, framePtr, 5)) {
-						framePtr += 5;	/* eliminate the SNAP header */
-
-						ea = (struct elapaarp *)framePtr;
-					} else if (!memcmp(ddp_snap_id, framePtr, 5)) {
-						framePtr += 5;	/* eliminate the SNAP header */
-
-						ddp = (struct ddpehdr *)framePtr;
-					} else {
-						DEBUG_WARN("NAT25: Protocol=Ethernet SNAP %02x%02x%02x%02x%02x\n", framePtr[0],
-							framePtr[1], framePtr[2], framePtr[3], framePtr[4]);
-						return -1;
-					}
-				} else if (*framePtr == ipx_8022_type) {
-					framePtr += 3;	/* eliminate the 802.2 header */
-
-					if (!memcmp(ipx_header, framePtr, 2)) {
-						RTW_INFO("NAT25: Protocol=IPX (Ethernet 802.2)\n");
-						ipx = (struct ipxhdr *)framePtr;
-					} else
-						return -1;
-				}
-			}
-		}
-
-		/*   IPX  */
-		if (ipx != NULL) {
-			switch (method) {
-			case NAT25_CHECK:
-				if (!memcmp(skb->data + ETH_ALEN, ipx->ipx_source.node, ETH_ALEN)) {
-					RTW_INFO("NAT25: Check IPX skb_copy\n");
-					return 0;
-				}
-				return -1;
-
-			case NAT25_INSERT: {
-				RTW_INFO("NAT25: Insert IPX, Dest=%08x,%02x%02x%02x%02x%02x%02x,%04x Source=%08x,%02x%02x%02x%02x%02x%02x,%04x\n",
-					 ipx->ipx_dest.net,
-					 ipx->ipx_dest.node[0],
-					 ipx->ipx_dest.node[1],
-					 ipx->ipx_dest.node[2],
-					 ipx->ipx_dest.node[3],
-					 ipx->ipx_dest.node[4],
-					 ipx->ipx_dest.node[5],
-					 ipx->ipx_dest.sock,
-					 ipx->ipx_source.net,
-					 ipx->ipx_source.node[0],
-					 ipx->ipx_source.node[1],
-					 ipx->ipx_source.node[2],
-					 ipx->ipx_source.node[3],
-					 ipx->ipx_source.node[4],
-					 ipx->ipx_source.node[5],
-					 ipx->ipx_source.sock);
-
-				if (!memcmp(skb->data + ETH_ALEN, ipx->ipx_source.node, ETH_ALEN)) {
-					RTW_INFO("NAT25: Use IPX Net, and Socket as network addr\n");
-
-					__nat25_generate_ipx_network_addr_with_socket(networkAddr, &ipx->ipx_source.net, &ipx->ipx_source.sock);
-
-					/* change IPX source node addr to wlan STA address */
-					memcpy(ipx->ipx_source.node, GET_MY_HWADDR(priv), ETH_ALEN);
-				} else
-					__nat25_generate_ipx_network_addr_with_node(networkAddr, &ipx->ipx_source.net, ipx->ipx_source.node);
-
-				__nat25_db_network_insert(priv, skb->data + ETH_ALEN, networkAddr);
-
-				__nat25_db_print(priv);
-			}
-			return 0;
-
-			case NAT25_LOOKUP: {
-				if (!memcmp(GET_MY_HWADDR(priv), ipx->ipx_dest.node, ETH_ALEN)) {
-					RTW_INFO("NAT25: Lookup IPX, Modify Destination IPX Node addr\n");
-
-					__nat25_generate_ipx_network_addr_with_socket(networkAddr, &ipx->ipx_dest.net, &ipx->ipx_dest.sock);
-
-					__nat25_db_network_lookup_and_replace(priv, skb, networkAddr);
-
-					/* replace IPX destination node addr with Lookup destination MAC addr */
-					memcpy(ipx->ipx_dest.node, skb->data, ETH_ALEN);
-				} else {
-					__nat25_generate_ipx_network_addr_with_node(networkAddr, &ipx->ipx_dest.net, ipx->ipx_dest.node);
-
-					__nat25_db_network_lookup_and_replace(priv, skb, networkAddr);
-				}
-			}
-			return 0;
-
-			default:
-				return -1;
-			}
-		}
-
-		/*   AARP  */
-		else if (ea != NULL) {
-			/* Sanity check fields. */
-			if (ea->hw_len != ETH_ALEN || ea->pa_len != AARP_PA_ALEN) {
-				DEBUG_WARN("NAT25: Appletalk AARP Sanity check fail!\n");
-				return -1;
-			}
-
-			switch (method) {
-			case NAT25_CHECK:
-				return 0;
-
-			case NAT25_INSERT: {
-				/* change to AARP source mac address to wlan STA address */
-				memcpy(ea->hw_src, GET_MY_HWADDR(priv), ETH_ALEN);
-
-				RTW_INFO("NAT25: Insert AARP, Source=%d,%d Destination=%d,%d\n",
-					 ea->pa_src_net,
-					 ea->pa_src_node,
-					 ea->pa_dst_net,
-					 ea->pa_dst_node);
-
-				__nat25_generate_apple_network_addr(networkAddr, &ea->pa_src_net, &ea->pa_src_node);
-
-				__nat25_db_network_insert(priv, skb->data + ETH_ALEN, networkAddr);
-
-				__nat25_db_print(priv);
-			}
-			return 0;
-
-			case NAT25_LOOKUP: {
-				RTW_INFO("NAT25: Lookup AARP, Source=%d,%d Destination=%d,%d\n",
-					 ea->pa_src_net,
-					 ea->pa_src_node,
-					 ea->pa_dst_net,
-					 ea->pa_dst_node);
-
-				__nat25_generate_apple_network_addr(networkAddr, &ea->pa_dst_net, &ea->pa_dst_node);
-
-				__nat25_db_network_lookup_and_replace(priv, skb, networkAddr);
-
-				/* change to AARP destination mac address to Lookup result */
-				memcpy(ea->hw_dst, skb->data, ETH_ALEN);
-			}
-			return 0;
-
-			default:
-				return -1;
-			}
-		}
-
-		/*   DDP  */
-		else if (ddp != NULL) {
-			switch (method) {
-			case NAT25_CHECK:
-				return -1;
-
-			case NAT25_INSERT: {
-				RTW_INFO("NAT25: Insert DDP, Source=%d,%d Destination=%d,%d\n",
-					 ddp->deh_snet,
-					 ddp->deh_snode,
-					 ddp->deh_dnet,
-					 ddp->deh_dnode);
-
-				__nat25_generate_apple_network_addr(networkAddr, &ddp->deh_snet, &ddp->deh_snode);
-
-				__nat25_db_network_insert(priv, skb->data + ETH_ALEN, networkAddr);
-
-				__nat25_db_print(priv);
-			}
-			return 0;
-
-			case NAT25_LOOKUP: {
-				RTW_INFO("NAT25: Lookup DDP, Source=%d,%d Destination=%d,%d\n",
-					 ddp->deh_snet,
-					 ddp->deh_snode,
-					 ddp->deh_dnet,
-					 ddp->deh_dnode);
-
-				__nat25_generate_apple_network_addr(networkAddr, &ddp->deh_dnet, &ddp->deh_dnode);
-
-				__nat25_db_network_lookup_and_replace(priv, skb, networkAddr);
-			}
-			return 0;
-
-			default:
-				return -1;
-			}
-		}
-
-		return -1;
-	}
-
 	/*---------------------------------------------------*/
 	/*                Handle PPPoE frame                */
 	/*---------------------------------------------------*/
-- 
2.46.0

