From c72c45ebf95d361086a5d0fc7022e59ad86c2f5b Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Mon, 26 Apr 2021 01:31:27 +0200
Subject: [PATCH 180/463] arm64: dts: sun50i-a64-pinephone: Don't make lradc
 keys a wakeup source

This allow the crust to reach lower suspend state.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
index b64b3b65997a8..0a8352147280a 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
@@ -540,7 +540,7 @@ &i2s2 {
 
 &lradc {
 	vref-supply = <&reg_aldo3>;
-	wakeup-source;
+//	wakeup-source;
 	status = "okay";
 
 	button-200 {
-- 
2.46.0

