From 5185b4267e3b526a8fa7914d0fe0d7ce9fc27ebd Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Kamil=20Trzci=C5=84ski?= <ayufan@ayufan.eu>
Date: Mon, 4 Jan 2021 17:57:49 +0100
Subject: [PATCH 318/463] power: rk818: Configure `rk808-clkout2` function
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

???

Signed-of-by: Kamil Trzciński <ayufan@ayufan.eu>
---
 drivers/mfd/rk8xx-core.c  | 1 +
 include/linux/mfd/rk808.h | 2 ++
 2 files changed, 3 insertions(+)

diff --git a/drivers/mfd/rk8xx-core.c b/drivers/mfd/rk8xx-core.c
index 5eda3c0dbbdf1..95fe71faa77e2 100644
--- a/drivers/mfd/rk8xx-core.c
+++ b/drivers/mfd/rk8xx-core.c
@@ -281,6 +281,7 @@ static const struct rk808_reg_data rk818_pre_init_reg[] = {
 	{ RK818_H5V_EN_REG,	  BIT(0),	    RK818_H5V_EN },
 	{ RK808_VB_MON_REG,	  MASK_ALL,	    VB_LO_ACT |
 						    VB_LO_SEL_3500MV },
+	{ RK808_CLK32OUT_REG, CLK32KOUT2_FUNC_MASK, CLK32KOUT2_FUNC },
 };
 
 static const struct regmap_irq rk805_irqs[] = {
diff --git a/include/linux/mfd/rk808.h b/include/linux/mfd/rk808.h
index 69cbea78b430b..b9afafed4512f 100644
--- a/include/linux/mfd/rk808.h
+++ b/include/linux/mfd/rk808.h
@@ -932,6 +932,8 @@ enum rk806_dvs_mode {
 
 #define VOUT_LO_INT	BIT(0)
 #define CLK32KOUT2_EN	BIT(0)
+#define CLK32KOUT2_FUNC		(0 << 1)
+#define CLK32KOUT2_FUNC_MASK	BIT(1)
 
 #define TEMP105C			0x08
 #define TEMP115C			0x0c
-- 
2.46.0

