From a8ed0a53f1f50263fbc8e2ba8cba6f4edc878e27 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Wed, 23 Sep 2020 14:59:41 +0200
Subject: [PATCH 281/463] power: supply: axp20x_battery: Setup thermal
 regulation (experimental)

Values for NTC resistances were pulled out of thin air!

None of this is tested to actually work.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 drivers/power/supply/axp20x_battery.c | 54 +++++++++++++++++++++++++++
 1 file changed, 54 insertions(+)

diff --git a/drivers/power/supply/axp20x_battery.c b/drivers/power/supply/axp20x_battery.c
index bad981c349ff3..5aed07bbc716e 100644
--- a/drivers/power/supply/axp20x_battery.c
+++ b/drivers/power/supply/axp20x_battery.c
@@ -589,6 +589,7 @@ static int axp20x_power_probe(struct platform_device *pdev)
 	struct power_supply_config psy_cfg = {};
 	struct power_supply_battery_info *info;
 	struct device *dev = &pdev->dev;
+	int ret;
 
 	if (!of_device_is_available(pdev->dev.of_node))
 		return -ENODEV;
@@ -669,6 +670,59 @@ static int axp20x_power_probe(struct platform_device *pdev)
 	axp20x_get_constant_charge_current(axp20x_batt,
 					   &axp20x_batt->max_ccc);
 
+	if (of_machine_is_compatible("pine64,pinephone-1.2") > 0 ||
+		of_machine_is_compatible("pine64,pinephone-1.1") > 0 ||
+		of_machine_is_compatible("pine64,pinephone-1.0") > 0) {
+		// 3kOhm NTC inside PinePhone batery
+		// ---------------------------------
+		//
+		// Charging:
+		//  0 - 15 °C: Max 0.2C CC to 4.35V : 9750 Ohm - 4710 Ohm
+		// 15 - 50 °C: Max 0.5C CC to 4.35V : 4710 Ohm - 1080 Ohm
+		//
+		// Discharging:
+		// -10 °C : 16500 Ohm
+		//  55 °C : 896 Ohm
+		// enable TS pin input to ADC
+
+		dev_info(dev, "Configuring battery thermal regulation for Pinephone\n");
+
+		ret = regmap_update_bits(axp20x_batt->regmap, 0x82, BIT(0), BIT(0));
+		if (ret)
+			goto warn_bat;
+
+		// safety thresholds:
+
+		// voltage = reg_val * 12800 uV (range is 0 - 3.264V)
+		ret = regmap_write(axp20x_batt->regmap, 0x38,  9750 * 80 / 12800); // V_LTF-charge
+		if (ret)
+			goto warn_bat;
+
+		ret = regmap_write(axp20x_batt->regmap, 0x39,  1080 * 80 / 12800); // V_HTF-charge
+		if (ret)
+			goto warn_bat;
+
+		ret = regmap_write(axp20x_batt->regmap, 0x3c, 16500 * 80 / 12800); // V_LTF-work
+		if (ret)
+			goto warn_bat;
+
+		ret = regmap_write(axp20x_batt->regmap, 0x3d,   896 * 80 / 12800); // V_HTF-work
+		if (ret)
+			goto warn_bat;
+
+		// There is a hysteresis of 460.8 mV(refer to TS pin voltage) for UTP
+		// threshold, and there is a hysteresis of 57.6 mV for OTP threshold.
+
+		// use TS pin only when charging, make it affect the charger, I = 80uA
+		ret = regmap_update_bits(axp20x_batt->regmap, 0x84, 0x37, 0x31);
+		if (ret)
+			goto warn_bat;
+	}
+
+	return 0;
+
+warn_bat:
+	dev_err(dev, "Failed to configure battery thermal regulation\n");
 	return 0;
 }
 
-- 
2.46.0

