From 7b344d06b54ac85384e0fbd6bc2e6b235cb69783 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Mon, 29 May 2023 21:35:22 +0200
Subject: [PATCH 387/463] arm64: dts: rk3399-pinephone-pro: Fix voltage
 threshold for volume down key

U-Boot and Linux use different algorithms for determining voltage ranges
for comparison. Pick value that will work with both.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts b/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
index 7f4dd9f1ae0d9..b06d0b0bda541 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3399-pinephone-pro.dts
@@ -48,7 +48,7 @@ button-up {
 		button-down {
 			label = "Volume Down";
 			linux,code = <KEY_VOLUMEDOWN>;
-			press-threshold-microvolt = <600000>;
+			press-threshold-microvolt = <400000>;
 		};
 	};
 
-- 
2.46.0

