From 762d8c40e9ea4a5898cb8fc6127a56b566d73f81 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Fri, 29 Jul 2022 01:08:29 +0200
Subject: [PATCH 242/463] ASoC: codec: es8316: "DAC Soft Ramp Rate" is just a 2
 bit control

Max value should be 3, otherwise "DAC Soft Ramp Switch" will be
overwritten by this control.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 sound/soc/codecs/es8316.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/sound/soc/codecs/es8316.c b/sound/soc/codecs/es8316.c
index 61729e5b50a8e..71aad3e4c83f8 100644
--- a/sound/soc/codecs/es8316.c
+++ b/sound/soc/codecs/es8316.c
@@ -99,7 +99,7 @@ static const struct snd_kcontrol_new es8316_snd_controls[] = {
 	SOC_DOUBLE_R_TLV("DAC Playback Volume", ES8316_DAC_VOLL,
 			 ES8316_DAC_VOLR, 0, 0xc0, 1, dac_vol_tlv),
 	SOC_SINGLE("DAC Soft Ramp Switch", ES8316_DAC_SET1, 4, 1, 1),
-	SOC_SINGLE("DAC Soft Ramp Rate", ES8316_DAC_SET1, 2, 4, 0),
+	SOC_SINGLE("DAC Soft Ramp Rate", ES8316_DAC_SET1, 2, 3, 0),
 	SOC_SINGLE("DAC Notch Filter Switch", ES8316_DAC_SET2, 6, 1, 0),
 	SOC_SINGLE("DAC Double Fs Switch", ES8316_DAC_SET2, 7, 1, 0),
 	SOC_SINGLE("DAC Stereo Enhancement", ES8316_DAC_SET3, 0, 7, 0),
-- 
2.46.0

