From a8bbda5905005e0dbbf21ba3518d381accbf3333 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Sat, 18 Nov 2023 00:30:56 +0100
Subject: [PATCH 047/463] 8723cs: Port to linux 6.7

---
 drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c b/drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c
index c1e6e9eff9b3b..817041e4644b5 100644
--- a/drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c
+++ b/drivers/staging/rtl8723cs/os_dep/linux/ioctl_cfg80211.c
@@ -5336,10 +5336,11 @@ static int cfg80211_rtw_start_ap(struct wiphy *wiphy, struct net_device *ndev,
 }
 
 static int cfg80211_rtw_change_beacon(struct wiphy *wiphy, struct net_device *ndev,
-		struct cfg80211_beacon_data *info)
+				      struct cfg80211_ap_update *params)
 {
 	int ret = 0;
 	_adapter *adapter = (_adapter *)rtw_netdev_priv(ndev);
+	struct cfg80211_beacon_data *info = &params->beacon;
 
 	RTW_INFO(FUNC_NDEV_FMT"\n", FUNC_NDEV_ARG(ndev));
 
-- 
2.46.0

