From 54792029656a07b4a208ce7b94a5313cb706ebc4 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sun, 21 Nov 2021 17:01:48 +0100
Subject: [PATCH 231/463] arm64: dts: rk3399-pinebook-pro: Remove redundant
 pinctrl-* properties from edp

These are already present in rk3399.dtsi.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/rockchip/rk3399-pinebook-pro.dts | 2 --
 1 file changed, 2 deletions(-)

diff --git a/arch/arm64/boot/dts/rockchip/rk3399-pinebook-pro.dts b/arch/arm64/boot/dts/rockchip/rk3399-pinebook-pro.dts
index 62e9e85b16d51..8e959085e2304 100644
--- a/arch/arm64/boot/dts/rockchip/rk3399-pinebook-pro.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3399-pinebook-pro.dts
@@ -402,8 +402,6 @@ &cpu_l3 {
 
 &edp {
 	force-hpd;
-	pinctrl-names = "default";
-	pinctrl-0 = <&edp_hpd>;
 	status = "okay";
 
 	ports {
-- 
2.46.0

