From e84e2fb52a234b8f646fb10450ddc64477d4047d Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Sun, 16 Oct 2022 23:20:59 +0200
Subject: [PATCH 240/463] arm64: dts: sun50i-a64: Add missing trip points for
 GPU

Linux 6.1 requires them.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi | 18 ++++++++++++++++++
 1 file changed, 18 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index e868ca5ae753a..12ad897fa61fc 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -263,6 +263,15 @@ gpu0_thermal: gpu0-thermal {
 			polling-delay-passive = <0>;
 			polling-delay = <0>;
 			thermal-sensors = <&ths 1>;
+
+			trips {
+				gpu0_crit: gpu-crit {
+					/* milliCelsius */
+					temperature = <110000>;
+					hysteresis = <2000>;
+					type = "critical";
+				};
+			};
 		};
 
 		gpu1_thermal: gpu1-thermal {
@@ -270,6 +279,15 @@ gpu1_thermal: gpu1-thermal {
 			polling-delay-passive = <0>;
 			polling-delay = <0>;
 			thermal-sensors = <&ths 2>;
+
+			trips {
+				gpu1_crit: gpu-crit {
+					/* milliCelsius */
+					temperature = <110000>;
+					hysteresis = <2000>;
+					type = "critical";
+				};
+			};
 		};
 	};
 
-- 
2.46.0

